###############################################################
# JP2 codestream log file generated by jp2codestream.py       #
# jp2codestream.py is copyrighted (c) 2001,2002               #
# by Algo Vision Technology GmbH, All Rights Reserved         #
#                                                             #
# http://www.av-technology.de/ jpeg2000@av-technology.de      #
###############################################################

0       : New marker: SOC (Start of codestream)

2       : New marker: SIZ (Image and tile size)

  Required Capabilities          : JPEG2000 profile 0
  Reference Grid Size            : 256x256
  Image Offset                   : 0x0
  Reference Tile Size            : 128x128
  Reference Tile Offset          : 0x0
  Components                     : 1
  Component #0 Depth             : 4
  Component #0 Signed            : yes
  Component #0 Sample Separation : 1x1

45      : New marker: COD (Coding style default)

  Default Precincts of 2^15x2^15     : yes
  SOP Marker Segments                : yes
  EPH Marker Segments                : no
  All Flags                          : 00000002
  Progression Order                  : position-component-resolution level-layer
  Layers                             : 8
  Multiple Component Transformation  : none
  Decomposition Levels               : 1
  Code-block size                    : 64x64
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : no
  Vertically Causal Context          : no
  Predictable Termination            : no
  Segmentation Symbols               : no
  Wavelet Transformation             : 5-3 reversible

59      : New marker: QCD (Quantization default)

  Quantization Type : scalar derived
  Guard Bits        : 2
  Mantissa #0       : 0
  Exponent #0       : 0

66      : New marker: QCC (Quantization component)

  Index             : 0
  Quantization Type : none
  Guard Bits        : 2
  Exponent #0       : 4
  Exponent #1       : 5
  Exponent #2       : 5
  Exponent #3       : 6

76      : New marker: POC (Progression order change)

  Resolution Level Index #0 (Start) : 0
  Component Index #0 (Start)        : 0
  Layer Index #0 (End)              : 8
  Resolution Level Index #0 (End)   : 33
  Component Index #0 (End)          : 255
  Progression Order #0              : layer-resolution level-component-position

87      : New marker: CRG (Component registration)

  Offset #0 : 65424x32558

95      : New marker: COM (Comment)

  Registration : ISO-8859-15
  Comment      : Creator: AV-J2K (c) 2000,2001 Algo Vision

142     : New marker: COM (Comment)

  Registration : ISO-8859-15
  Comment      : Creator: AV-J2K (c) 2000,2001 Algo Vision Technology

200     : New marker: COM (Comment)

  Registration : binary
  Comment      : ...

268     : New marker: TLM (Tile-part length)

  Index         : 0
  Tile index #0 : 0
  Length #0     : 4267
  Tile index #1 : 1
  Length #1     : 2117
  Tile index #2 : 2
  Length #2     : 4080
  Tile index #3 : 3
  Length #3     : 2081

298     : New marker: SOT (Start of tile-part)

  Tile        : 0
  Length      : 4267
  Index       : 0
  Tile-Parts: : 1

310     : New marker: RGN (Region-of-interest)

  Component          : 0
  Style              : implicit
  Implicit ROI Shift : 7

317     : New marker: SOD (Start of data)

319     : New marker: SOP (Start of packet)

  Sequence : 0

Data : 245 bytes

570     : New marker: SOP (Start of packet)

  Sequence : 1

Data : 225 bytes

801     : New marker: SOP (Start of packet)

  Sequence : 2

Data : 1 bytes

808     : New marker: SOP (Start of packet)

  Sequence : 3

Data : 208 bytes

1022    : New marker: SOP (Start of packet)

  Sequence : 4

Data : 359 bytes

1387    : New marker: SOP (Start of packet)

  Sequence : 5

Data : 55 bytes

1448    : New marker: SOP (Start of packet)

  Sequence : 6

Data : 71 bytes

1525    : New marker: SOP (Start of packet)

  Sequence : 7

Data : 24 bytes

1555    : New marker: SOP (Start of packet)

  Sequence : 8

Data : 831 bytes

2392    : New marker: SOP (Start of packet)

  Sequence : 9

Data : 582 bytes

2980    : New marker: SOP (Start of packet)

  Sequence : 10

Data : 1 bytes

2987    : New marker: SOP (Start of packet)

  Sequence : 11

Data : 1295 bytes

4288    : New marker: SOP (Start of packet)

  Sequence : 12

Data : 1 bytes

4295    : New marker: SOP (Start of packet)

  Sequence : 13

Data : 250 bytes

4551    : New marker: SOP (Start of packet)

  Sequence : 14

Data : 1 bytes

4558    : New marker: SOP (Start of packet)

  Sequence : 15

Data : 1 bytes

4565    : New marker: SOT (Start of tile-part)

  Tile        : 1
  Length      : 2117
  Index       : 0
  Tile-Parts: : 1

4577    : New marker: SOD (Start of data)

4579    : New marker: SOP (Start of packet)

  Sequence : 0

Data : 63 bytes

4648    : New marker: SOP (Start of packet)

  Sequence : 1

Data : 1 bytes

4655    : New marker: SOP (Start of packet)

  Sequence : 2

Data : 1 bytes

4662    : New marker: SOP (Start of packet)

  Sequence : 3

Data : 1 bytes

4669    : New marker: SOP (Start of packet)

  Sequence : 4

Data : 156 bytes

4831    : New marker: SOP (Start of packet)

  Sequence : 5

Data : 1 bytes

4838    : New marker: SOP (Start of packet)

  Sequence : 6

Data : 59 bytes

4903    : New marker: SOP (Start of packet)

  Sequence : 7

Data : 1 bytes

4910    : New marker: SOP (Start of packet)

  Sequence : 8

Data : 498 bytes

5414    : New marker: SOP (Start of packet)

  Sequence : 9

Data : 1 bytes

5421    : New marker: SOP (Start of packet)

  Sequence : 10

Data : 1 bytes

5428    : New marker: SOP (Start of packet)

  Sequence : 11

Data : 790 bytes

6224    : New marker: SOP (Start of packet)

  Sequence : 12

Data : 1 bytes

6231    : New marker: SOP (Start of packet)

  Sequence : 13

Data : 431 bytes

6668    : New marker: SOP (Start of packet)

  Sequence : 14

Data : 1 bytes

6675    : New marker: SOP (Start of packet)

  Sequence : 15

Data : 1 bytes

6682    : New marker: SOT (Start of tile-part)

  Tile        : 2
  Length      : 4080
  Index       : 0
  Tile-Parts: : 1

6694    : New marker: SOD (Start of data)

6696    : New marker: SOP (Start of packet)

  Sequence : 0

Data : 191 bytes

6893    : New marker: SOP (Start of packet)

  Sequence : 1

Data : 1 bytes

6900    : New marker: SOP (Start of packet)

  Sequence : 2

Data : 1 bytes

6907    : New marker: SOP (Start of packet)

  Sequence : 3

Data : 1 bytes

6914    : New marker: SOP (Start of packet)

  Sequence : 4

Data : 1 bytes

6921    : New marker: SOP (Start of packet)

  Sequence : 5

Data : 1 bytes

6928    : New marker: SOP (Start of packet)

  Sequence : 6

Data : 248 bytes

7182    : New marker: SOP (Start of packet)

  Sequence : 7

Data : 1 bytes

7189    : New marker: SOP (Start of packet)

  Sequence : 8

Data : 604 bytes

7799    : New marker: SOP (Start of packet)

  Sequence : 9

Data : 71 bytes

7876    : New marker: SOP (Start of packet)

  Sequence : 10

Data : 421 bytes

8303    : New marker: SOP (Start of packet)

  Sequence : 11

Data : 2084 bytes

10393   : New marker: SOP (Start of packet)

  Sequence : 12

Data : 1 bytes

10400   : New marker: SOP (Start of packet)

  Sequence : 13

Data : 342 bytes

10748   : New marker: SOP (Start of packet)

  Sequence : 14

Data : 1 bytes

10755   : New marker: SOP (Start of packet)

  Sequence : 15

Data : 1 bytes

10762   : New marker: SOT (Start of tile-part)

  Tile        : 3
  Length      : 2081
  Index       : 0
  Tile-Parts: : 1

10774   : New marker: SOD (Start of data)

10776   : New marker: SOP (Start of packet)

  Sequence : 0

Data : 1 bytes

10783   : New marker: SOP (Start of packet)

  Sequence : 1

Data : 93 bytes

10882   : New marker: SOP (Start of packet)

  Sequence : 2

Data : 1 bytes

10889   : New marker: SOP (Start of packet)

  Sequence : 3

Data : 1 bytes

10896   : New marker: SOP (Start of packet)

  Sequence : 4

Data : 282 bytes

11184   : New marker: SOP (Start of packet)

  Sequence : 5

Data : 1 bytes

11191   : New marker: SOP (Start of packet)

  Sequence : 6

Data : 1 bytes

11198   : New marker: SOP (Start of packet)

  Sequence : 7

Data : 1 bytes

11205   : New marker: SOP (Start of packet)

  Sequence : 8

Data : 475 bytes

11686   : New marker: SOP (Start of packet)

  Sequence : 9

Data : 1 bytes

11693   : New marker: SOP (Start of packet)

  Sequence : 10

Data : 1 bytes

11700   : New marker: SOP (Start of packet)

  Sequence : 11

Data : 675 bytes

12381   : New marker: SOP (Start of packet)

  Sequence : 12

Data : 1 bytes

12388   : New marker: SOP (Start of packet)

  Sequence : 13

Data : 435 bytes

12829   : New marker: SOP (Start of packet)

  Sequence : 14

Data : 1 bytes

12836   : New marker: SOP (Start of packet)

  Sequence : 15

Data : 1 bytes

12843   : New marker: EOC (End of codestream)

Size: 12845 bytes
Data Size: 12098 bytes
Overhead: 747 bytes (5%)
