###############################################################
# JP2 codestream log file generated by jp2codestream.py       #
# jp2codestream.py is copyrighted (c) 2001,2002               #
# by Algo Vision Technology GmbH, All Rights Reserved         #
#                                                             #
# http://www.av-technology.de/ jpeg2000@av-technology.de      #
###############################################################

0       : New marker: SOC (Start of codestream)

2       : New marker: SIZ (Image and tile size)

  Required Capabilities          : JPEG2000 profile 1
  Reference Grid Size            : 12x12
  Image Offset                   : 4x0
  Reference Tile Size            : 12x12
  Reference Tile Offset          : 4x0
  Components                     : 2
  Component #0 Depth             : 8
  Component #0 Signed            : no
  Component #0 Sample Separation : 4x1
  Component #1 Depth             : 8
  Component #1 Signed            : no
  Component #1 Sample Separation : 1x1

48      : New marker: COD (Coding style default)

  Default Precincts of 2^15x2^15     : no
  SOP Marker Segments                : yes
  EPH Marker Segments                : yes
  All Flags                          : 00000007
  Progression Order                  : resolution level-position-component-layer
  Layers                             : 1
  Multiple Component Transformation  : none
  Decomposition Levels               : 1
  Code-block size                    : 64x64
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : no
  Vertically Causal Context          : no
  Predictable Termination            : no
  Segmentation Symbols               : no
  Wavelet Transformation             : 5-3 reversible
  Precinct #0 Size Exponents         : 0x0
  Precinct #1 Size Exponents         : 1x1

64      : New marker: COC (Coding style component)

  Component                          : 1
  Precincts                          : custom
  Decomposition Levels               : 1
  Code-block size                    : 64x64
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : no
  Vertically Causal Context          : no
  Predictable Termination            : no
  Segmentation Symbols               : no
  Wavelet Transformation             : 5-3 reversible
  Precinct #0 Size Exponents         : 1x1
  Precinct #1 Size Exponents         : 2x2

77      : New marker: QCD (Quantization default)

  Quantization Type : none
  Guard Bits        : 2
  Exponent #0       : 8
  Exponent #1       : 9
  Exponent #2       : 9
  Exponent #3       : 10

86      : New marker: COM (Comment)

  Registration : ISO-8859-15
  Comment      : Creator: AV-J2K (c) 2000,2001 Algo Vision

133     : New marker: SOT (Start of tile-part)

  Tile        : 0
  Length      : 434
  Index       : 0
  Tile-Parts: : 1

145     : New marker: SOD (Start of data)

147     : New marker: SOP (Start of packet)

  Sequence : 0

Data : 3 bytes

156     : New marker: EPH (End of packet header)

Data : 5 bytes

163     : New marker: SOP (Start of packet)

  Sequence : 1

Data : 3 bytes

172     : New marker: EPH (End of packet header)

Data : 1 bytes

175     : New marker: SOP (Start of packet)

  Sequence : 2

Data : 3 bytes

184     : New marker: EPH (End of packet header)

Data : 5 bytes

191     : New marker: SOP (Start of packet)

  Sequence : 3

Data : 3 bytes

200     : New marker: EPH (End of packet header)

Data : 1 bytes

203     : New marker: SOP (Start of packet)

  Sequence : 4

Data : 3 bytes

212     : New marker: EPH (End of packet header)

Data : 5 bytes

219     : New marker: SOP (Start of packet)

  Sequence : 5

Data : 3 bytes

228     : New marker: EPH (End of packet header)

Data : 1 bytes

231     : New marker: SOP (Start of packet)

  Sequence : 6

Data : 3 bytes

240     : New marker: EPH (End of packet header)

Data : 5 bytes

247     : New marker: SOP (Start of packet)

  Sequence : 7

Data : 3 bytes

256     : New marker: EPH (End of packet header)

Data : 1 bytes

259     : New marker: SOP (Start of packet)

  Sequence : 8

Data : 3 bytes

268     : New marker: EPH (End of packet header)

Data : 3 bytes

273     : New marker: SOP (Start of packet)

  Sequence : 9

Data : 3 bytes

282     : New marker: EPH (End of packet header)

Data : 1 bytes

285     : New marker: SOP (Start of packet)

  Sequence : 10

Data : 3 bytes

294     : New marker: EPH (End of packet header)

Data : 3 bytes

299     : New marker: SOP (Start of packet)

  Sequence : 11

Data : 3 bytes

308     : New marker: EPH (End of packet header)

Data : 1 bytes

311     : New marker: SOP (Start of packet)

  Sequence : 12

Data : 3 bytes

320     : New marker: EPH (End of packet header)

Data : 1 bytes

323     : New marker: SOP (Start of packet)

  Sequence : 13

Data : 9 bytes

338     : New marker: EPH (End of packet header)

Data : 11 bytes

351     : New marker: SOP (Start of packet)

  Sequence : 14

Data : 1 bytes

358     : New marker: EPH (End of packet header)

360     : New marker: SOP (Start of packet)

  Sequence : 15

Data : 9 bytes

375     : New marker: EPH (End of packet header)

Data : 12 bytes

389     : New marker: SOP (Start of packet)

  Sequence : 16

Data : 3 bytes

398     : New marker: EPH (End of packet header)

Data : 1 bytes

401     : New marker: SOP (Start of packet)

  Sequence : 17

Data : 1 bytes

408     : New marker: EPH (End of packet header)

410     : New marker: SOP (Start of packet)

  Sequence : 18

Data : 3 bytes

419     : New marker: EPH (End of packet header)

Data : 1 bytes

422     : New marker: SOP (Start of packet)

  Sequence : 19

Data : 9 bytes

437     : New marker: EPH (End of packet header)

Data : 7 bytes

446     : New marker: SOP (Start of packet)

  Sequence : 20

Data : 1 bytes

453     : New marker: EPH (End of packet header)

455     : New marker: SOP (Start of packet)

  Sequence : 21

Data : 4 bytes

465     : New marker: EPH (End of packet header)

Data : 5 bytes

472     : New marker: SOP (Start of packet)

  Sequence : 22

Data : 3 bytes

481     : New marker: EPH (End of packet header)

Data : 1 bytes

484     : New marker: SOP (Start of packet)

  Sequence : 23

Data : 1 bytes

491     : New marker: EPH (End of packet header)

493     : New marker: SOP (Start of packet)

  Sequence : 24

Data : 3 bytes

502     : New marker: EPH (End of packet header)

Data : 1 bytes

505     : New marker: SOP (Start of packet)

  Sequence : 25

Data : 4 bytes

515     : New marker: EPH (End of packet header)

Data : 3 bytes

520     : New marker: SOP (Start of packet)

  Sequence : 26

Data : 1 bytes

527     : New marker: EPH (End of packet header)

529     : New marker: SOP (Start of packet)

  Sequence : 27

Data : 4 bytes

539     : New marker: EPH (End of packet header)

Data : 5 bytes

546     : New marker: SOP (Start of packet)

  Sequence : 28

Data : 3 bytes

555     : New marker: EPH (End of packet header)

Data : 1 bytes

558     : New marker: SOP (Start of packet)

  Sequence : 29

Data : 1 bytes

565     : New marker: EPH (End of packet header)

567     : New marker: EOC (End of codestream)

Size: 569 bytes
Data Size: 180 bytes
Overhead: 389 bytes (68%)
