###############################################################
# JP2 codestream log file generated by jp2codestream.py       #
# jp2codestream.py is copyrighted (c) 2001,2002               #
# by Algo Vision Technology GmbH, All Rights Reserved         #
#                                                             #
# http://www.av-technology.de/ jpeg2000@av-technology.de      #
###############################################################

0       : New marker: SOC (Start of codestream)

2       : New marker: SIZ (Image and tile size)

  Required Capabilities          : JPEG2000 profile 1
  Reference Grid Size            : 127x227
  Image Offset                   : 5x128
  Reference Tile Size            : 127x126
  Reference Tile Offset          : 1x101
  Components                     : 1
  Component #0 Depth             : 8
  Component #0 Signed            : no
  Component #0 Sample Separation : 2x1

45      : New marker: COD (Coding style default)

  Default Precincts of 2^15x2^15     : yes
  SOP Marker Segments                : yes
  EPH Marker Segments                : yes
  All Flags                          : 00000006
  Progression Order                  : layer-resolution level-component-position
  Layers                             : 5
  Multiple Component Transformation  : none
  Decomposition Levels               : 3
  Code-block size                    : 64x64
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : yes
  Vertically Causal Context          : no
  Predictable Termination            : yes
  Segmentation Symbols               : yes
  Wavelet Transformation             : 9-7 irreversible

59      : New marker: COC (Coding style component)

  Component                          : 0
  Precincts                          : default
  Decomposition Levels               : 3
  Code-block size                    : 32x32
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : yes
  Vertically Causal Context          : no
  Predictable Termination            : yes
  Segmentation Symbols               : yes
  Wavelet Transformation             : 5-3 reversible

70      : New marker: QCD (Quantization default)

  Quantization Type : none
  Guard Bits        : 3
  Exponent #0       : 8
  Exponent #1       : 9
  Exponent #2       : 9
  Exponent #3       : 10
  Exponent #4       : 9
  Exponent #5       : 9
  Exponent #6       : 10
  Exponent #7       : 9
  Exponent #8       : 9
  Exponent #9       : 10

85      : New marker: COM (Comment)

  Registration : ISO-8859-15
  Comment      : Creator: AV-J2K (c) 2000,2001 Algo Vision

132     : New marker: SOT (Start of tile-part)

  Tile        : 0
  Length      : 4627
  Index       : 0
  Tile-Parts: : 1

144     : New marker: SOD (Start of data)

146     : New marker: SOP (Start of packet)

  Sequence : 0

Data : 6 bytes

158     : New marker: EPH (End of packet header)

Data : 41 bytes

201     : New marker: SOP (Start of packet)

  Sequence : 1

Data : 12 bytes

219     : New marker: EPH (End of packet header)

Data : 63 bytes

284     : New marker: SOP (Start of packet)

  Sequence : 2

Data : 4 bytes

294     : New marker: EPH (End of packet header)

Data : 55 bytes

351     : New marker: SOP (Start of packet)

  Sequence : 3

Data : 7 bytes

364     : New marker: EPH (End of packet header)

Data : 31 bytes

397     : New marker: SOP (Start of packet)

  Sequence : 4

Data : 1 bytes

404     : New marker: EPH (End of packet header)

406     : New marker: SOP (Start of packet)

  Sequence : 5

Data : 1 bytes

413     : New marker: EPH (End of packet header)

415     : New marker: SOP (Start of packet)

  Sequence : 6

Data : 1 bytes

422     : New marker: EPH (End of packet header)

424     : New marker: SOP (Start of packet)

  Sequence : 7

Data : 1 bytes

431     : New marker: EPH (End of packet header)

433     : New marker: SOP (Start of packet)

  Sequence : 8

Data : 3 bytes

442     : New marker: EPH (End of packet header)

Data : 17 bytes

461     : New marker: SOP (Start of packet)

  Sequence : 9

Data : 9 bytes

476     : New marker: EPH (End of packet header)

Data : 60 bytes

538     : New marker: SOP (Start of packet)

  Sequence : 10

Data : 11 bytes

555     : New marker: EPH (End of packet header)

Data : 126 bytes

683     : New marker: SOP (Start of packet)

  Sequence : 11

Data : 11 bytes

700     : New marker: EPH (End of packet header)

Data : 196 bytes

898     : New marker: SOP (Start of packet)

  Sequence : 12

Data : 6 bytes

910     : New marker: EPH (End of packet header)

Data : 43 bytes

955     : New marker: SOP (Start of packet)

  Sequence : 13

Data : 22 bytes

983     : New marker: EPH (End of packet header)

Data : 170 bytes

1155    : New marker: SOP (Start of packet)

  Sequence : 14

Data : 37 bytes

1198    : New marker: EPH (End of packet header)

Data : 756 bytes

1956    : New marker: SOP (Start of packet)

  Sequence : 15

Data : 85 bytes

2047    : New marker: EPH (End of packet header)

Data : 2674 bytes

4723    : New marker: SOP (Start of packet)

  Sequence : 16

Data : 1 bytes

4730    : New marker: EPH (End of packet header)

4732    : New marker: SOP (Start of packet)

  Sequence : 17

Data : 1 bytes

4739    : New marker: EPH (End of packet header)

4741    : New marker: SOP (Start of packet)

  Sequence : 18

Data : 1 bytes

4748    : New marker: EPH (End of packet header)

4750    : New marker: SOP (Start of packet)

  Sequence : 19

Data : 1 bytes

4757    : New marker: EPH (End of packet header)

4759    : New marker: EOC (End of codestream)

Size: 4761 bytes
Data Size: 4453 bytes
Overhead: 308 bytes (6%)
