###############################################################
# JP2 codestream log file generated by jp2codestream.py       #
# jp2codestream.py is copyrighted (c) 2001,2002               #
# by Algo Vision Technology GmbH, All Rights Reserved         #
#                                                             #
# http://www.av-technology.de/ jpeg2000@av-technology.de      #
###############################################################

0       : New marker: SOC (Start of codestream)

2       : New marker: SIZ (Image and tile size)

  Required Capabilities          : JPEG2000 profile 0
  Reference Grid Size            : 127x126
  Image Offset                   : 0x0
  Reference Tile Size            : 127x126
  Reference Tile Offset          : 0x0
  Components                     : 1
  Component #0 Depth             : 8
  Component #0 Signed            : no
  Component #0 Sample Separation : 2x1

45      : New marker: COD (Coding style default)

  Default Precincts of 2^15x2^15     : yes
  SOP Marker Segments                : yes
  EPH Marker Segments                : yes
  All Flags                          : 00000006
  Progression Order                  : layer-resolution level-component-position
  Layers                             : 6
  Multiple Component Transformation  : none
  Decomposition Levels               : 3
  Code-block size                    : 64x64
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : yes
  Vertically Causal Context          : no
  Predictable Termination            : yes
  Segmentation Symbols               : yes
  Wavelet Transformation             : 9-7 irreversible

59      : New marker: COC (Coding style component)

  Component                          : 0
  Precincts                          : default
  Decomposition Levels               : 3
  Code-block size                    : 32x32
  Selective Arithmetic Coding Bypass : no
  Reset Context Probabilities        : no
  Termination on Each Coding Pass    : yes
  Vertically Causal Context          : no
  Predictable Termination            : yes
  Segmentation Symbols               : yes
  Wavelet Transformation             : 5-3 reversible

70      : New marker: QCD (Quantization default)

  Quantization Type : none
  Guard Bits        : 3
  Exponent #0       : 8
  Exponent #1       : 9
  Exponent #2       : 9
  Exponent #3       : 10
  Exponent #4       : 9
  Exponent #5       : 9
  Exponent #6       : 10
  Exponent #7       : 9
  Exponent #8       : 9
  Exponent #9       : 10

85      : New marker: COM (Comment)

  Registration : ISO-8859-15
  Comment      : Creator: AV-J2K (c) 2000,2001 Algo Vision

132     : New marker: 0x30 (unknown segment-less)

134     : New marker: SOT (Start of tile-part)

  Tile        : 0
  Length      : 6047
  Index       : 0
  Tile-Parts: : 1

146     : New marker: SOD (Start of data)

148     : New marker: SOP (Start of packet)

  Sequence : 0

Data : 6 bytes

160     : New marker: EPH (End of packet header)

Data : 48 bytes

210     : New marker: SOP (Start of packet)

  Sequence : 1

Data : 9 bytes

225     : New marker: EPH (End of packet header)

Data : 42 bytes

269     : New marker: SOP (Start of packet)

  Sequence : 2

Data : 5 bytes

280     : New marker: EPH (End of packet header)

Data : 37 bytes

319     : New marker: SOP (Start of packet)

  Sequence : 3

Data : 5 bytes

330     : New marker: EPH (End of packet header)

Data : 20 bytes

352     : New marker: SOP (Start of packet)

  Sequence : 4

Data : 2 bytes

360     : New marker: EPH (End of packet header)

Data : 15 bytes

377     : New marker: SOP (Start of packet)

  Sequence : 5

Data : 1 bytes

384     : New marker: EPH (End of packet header)

386     : New marker: SOP (Start of packet)

  Sequence : 6

Data : 1 bytes

393     : New marker: EPH (End of packet header)

395     : New marker: SOP (Start of packet)

  Sequence : 7

Data : 1 bytes

402     : New marker: EPH (End of packet header)

404     : New marker: SOP (Start of packet)

  Sequence : 8

Data : 4 bytes

414     : New marker: EPH (End of packet header)

Data : 20 bytes

436     : New marker: SOP (Start of packet)

  Sequence : 9

Data : 11 bytes

453     : New marker: EPH (End of packet header)

Data : 82 bytes

537     : New marker: SOP (Start of packet)

  Sequence : 10

Data : 11 bytes

554     : New marker: EPH (End of packet header)

Data : 158 bytes

714     : New marker: SOP (Start of packet)

  Sequence : 11

Data : 10 bytes

730     : New marker: EPH (End of packet header)

Data : 157 bytes

889     : New marker: SOP (Start of packet)

  Sequence : 12

Data : 7 bytes

902     : New marker: EPH (End of packet header)

Data : 55 bytes

959     : New marker: SOP (Start of packet)

  Sequence : 13

Data : 22 bytes

987     : New marker: EPH (End of packet header)

Data : 195 bytes

1184    : New marker: SOP (Start of packet)

  Sequence : 14

Data : 24 bytes

1214    : New marker: EPH (End of packet header)

Data : 527 bytes

1743    : New marker: SOP (Start of packet)

  Sequence : 15

Data : 47 bytes

1796    : New marker: EPH (End of packet header)

Data : 1402 bytes

3200    : New marker: SOP (Start of packet)

  Sequence : 16

Data : 1 bytes

3207    : New marker: EPH (End of packet header)

3209    : New marker: SOP (Start of packet)

  Sequence : 17

Data : 9 bytes

3224    : New marker: EPH (End of packet header)

Data : 73 bytes

3299    : New marker: SOP (Start of packet)

  Sequence : 18

Data : 20 bytes

3325    : New marker: EPH (End of packet header)

Data : 521 bytes

3848    : New marker: SOP (Start of packet)

  Sequence : 19

Data : 51 bytes

3905    : New marker: EPH (End of packet header)

Data : 2238 bytes

6145    : New marker: SOP (Start of packet)

  Sequence : 20

Data : 1 bytes

6152    : New marker: EPH (End of packet header)

6154    : New marker: SOP (Start of packet)

  Sequence : 21

Data : 1 bytes

6161    : New marker: EPH (End of packet header)

6163    : New marker: SOP (Start of packet)

  Sequence : 22

Data : 1 bytes

6170    : New marker: EPH (End of packet header)

6172    : New marker: SOP (Start of packet)

  Sequence : 23

Data : 1 bytes

6179    : New marker: EPH (End of packet header)

6181    : New marker: EOC (End of codestream)

Size: 6183 bytes
Data Size: 5841 bytes
Overhead: 342 bytes (5%)
