# Dynamic Model for Stormwater Treatment Areas

## Documentation for package ‘DMSTAr’ version 0.1.1

- DESCRIPTION file
- User guides, package vignettes and other documentation
- Package NEWS
- Package README

## Help Pages

build_PSTA | Build parameter lists for supported DMSTAr models
build_P_kinetics | Build phosphorus kinetics parameters for a registered model
build_P_kin_slots | Build multi-slot phosphorus kinetics parameter vectors
build_RES | Build parameter lists for supported DMSTAr models
build_STA | Build parameter lists for supported DMSTAr models
cfs_to_hm3d | Convert Cubic Feet per Second to Cubic Hectometers per Day
dmstar_default_params | Create a default DMSTAr parameter list
dmsta_build_tanks | Build DMSTA tank partitioning for a cell
dmsta_cals | Parameter Sets for Stormwater Treatment Area Dynamic Model
dmsta_flowP_case | Run a networked DMSTA hydrology–phosphorus simulation
dmsta_flowP_series | Run a coupled hydrology–phosphorus simulation over a time series
dmsta_flow_series | Run a DMSTA hydrology simulation over a time series
dmsta_init_case_state | Initialize per-cell state for a network/case run
dmsta_make_cell | Create a DMSTA network cell definition
dmsta_p_init_state | Initialize DMSTA phosphorus state vectors for tanks
dmsta_validate_cells | Validate and normalize network cell definitions (internal)
model_parameter_builders | Build parameter lists for supported DMSTAr models
series | Example DMSTA daily forcing time series
validate_P_paramsK | Validate alignment of K-length phosphorus parameter vectors