// Copyright (C) 2020 The Qt Company Ltd.
// SPDX-License-Identifier: LicenseRef-Qt-Commercial OR GFDL-1.3-no-invariants-only

/*!
    \previouspage studio-javascript.html
    \page studio-simulink.html
    \nextpage creator-qml-modules-with-plugins.html

    \title Simulating dynamic systems

    Use the Simulink connector to connect simulation to your UI. Simulink is a
    MATLAB-based graphical programming environment for modeling, simulating,
    and analyzing multi-domain dynamic systems. On Windows, \QDS provides
    built-in support for connectivity to Simulink models, which allows them to
    send and receive data with applications developed using \QDS. Install
    Simulink on your computer and run it simultaneously with \QDS to enable
    communication between the applications.

    The information given here is mainly focused on the integration of the
    Simulink connector in \QDS. For information on how to use the Simulink
    environment, see the \l {https://se.mathworks.com/help/simulink/}
    {documentation} provided by MathWorks.

    \section1 The Qt Blockset for Simulink

    Install the Simulink \l {https://git.qt.io/design-studio/simulink/simulink-plugin-dependencies}
    {Qt Blockset} to your computer in order to connect a Simulink model to your
    application. The Qt Blockset installer adds the Simulink blocks needed to
    establish connectivity to your application. After installation, the
    \uicontrol SLQTLibrary blockset will be added to the Simulink blocks
    library. The blocks allow sending and receiving of \uicontrol Property,
    \uicontrol Signal, and \uicontrol Slot updates with your application. The
    Qt Blockset includes the \uicontrol {Simulink-Qt Client}, \uicontrol
    Address, \uicontrol {Qt/QML Send}, and \uicontrol {Qt/QML Receive} blocks.

    \image simulink-qt-blockset-receive.png "The Qt Blockset in a Simulink Model"

    \section2 Simulink-Qt Client

    A \uicontrol {Simulink-Qt Client} block establishes the TCP/IP Client
    connection with your application. The block has two inputs and two outputs:

    \list
        \li The \uicontrol Address input specifies the machine IP address
            of the server to the client block. To ensure the address is
            formatted correctly, use the \uicontrol Address block.
        \li The \uicontrol Port input specifies the port value for the IP
            address, which can be determined by using the \uicontrol Port block
            or a valid Simulink integer value.
        \li The \uicontrol IsConnected output is a Boolean signal. When true,
            specifies the connection to the server has been established.
        \li The \uicontrol Socket output sends a signal that presents the
            socket ID of the connection. This signal needs to be delivered to
            corresponding \uicontrol {Qt/QML Receive} and \uicontrol
            {Qt/QML Send} blocks.
    \endlist

    \section2 Address and port

    An \uicontrol Address block delivers the IP address of a server to the
    \uicontrol {Simulink-Qt Client} block as a typical IP address string.
    A \uicontrol Port block determines the port value for the IP address. For
    simulations where the Simulink model and your application are run on the
    same machine, use the IP address 127.0.0.1 and any port available.

    \section2 Qt/QML Send

    \image simulink-qt-send-block.png "A Qt/QML Send Block"

    A \uicontrol {Qt/QML Send} block sends a \uicontrol Signal or \uicontrol
    Property value change from Simulink. It is used for each property that
    Simulink needs to send to your application. The property name of the block
    needs to correspond to the name of the property or slot in your application.

    The block has two inputs and one output:
    \list
        \li The \uicontrol Socket input receives the socket signal from the
            \uicontrol {Simulink-Qt Client} block.
        \li The \uicontrol Data input receives the data to be sent as a
            \uicontrol Signal or \uicontrol Property update.
        \li The \uicontrol {Data Out} output outputs the passed-through data
            to connect it to other Simulink blocks if needed.
    \endlist

    \section2 Qt/QML Receive

    \image simulink-qt-receive-block.png "A Qt/QML Receive Block"

    A \uicontrol {Qt/QML Receive} block receives \uicontrol Signal or
    \uicontrol Property value changes from your application. It is used for
    each property that Simulink needs to receive from your application.
    The property name of the block needs to correspond to the name of the
    property or slot in your application.

   The block has one input and two outputs:

    \list
        \li The \uicontrol Socket input receives the socket signal from the
            \uicontrol {Simulink-Qt Client} block.
        \li The \uicontrol Fcn_Call output sends the function-call, which can
            either be terminated if idle, or connected to a valid function call
            subsystem.
        \li The \uicontrol isReceived output emits a scalar Boolean signal
            suggesting that a valid \uicontrol Signal or \uicontrol Property
            update was acquired from the connection.
        \li The \uicontrol Data output signals data payload from a \uicontrol
            Signal or \uicontrol Property value.
    \endlist

    \section2 Specifying property names in Simulink

    Double-click the \uicontrol {Qt/SML Send} or \uicontrol {Qt/QML Receive}
    block in Simulink to specify a property name. A pop-up for \uicontrol
    {Block Parameters} appears. Enter the name of the property in the \uicontrol
    {Qt Signal/Property Name} field and select \uicontrol OK. The name, for
    example speedProp, needs to match a \uicontrol signal or a \uicontrol
    property in \QDS.

    \image simulink-qt-send-example-property.png "Example property of the Qt Send block"

    \section1 Integrating the Simulink model to \QDS

    \section2 Importing the Simulink connector

    To integrate the Simulink model into \QDS, you first need to add the
    Simulink connector module to your project. In the \uicontrol Components
    view, select \imageplus
    > \uicontrol SimulinkConnector. \QDS is now ready to communicate with the
    Simulink model.

    \image studio-qml-imports-slconnector.png "Simulink Connector in the list of available modules."

    If you need to change the IP address and/or port, you need to select the
    \uicontrol SimulinkConnector item in \l Navigator and set the IP address
    and/or port in the \l Properties view. If you cannot see
    \uicontrol SimulinkConnector in \uicontrol Navigator, you need to click
    \imagefiltericon
    (\uicontrol {Filter Tree}) and unselect \uicontrol {Show only visible items}.

    To communicate with a specific model in Simulink, you need to create
    properties matching the send and receive properties in the root of the
    application you are building. Select the root item in \uicontrol
    Navigator to add the properties on the \uicontrol Properties tab in the
    \l Connections view.

    See \l {Specifying custom properties} for a detailed description of how
    to add a custom property. The name of the property and the data type
    need to match those of the send or receive property of the Simulink model.

    \image studio-connection-view-properties.png "The Properties tab in the Connections view"

    \section2 Creating bindings

    Next, you need to bind the value of the property you just created to the
    desired properties of UI components.

    By binding the root item property to a component property you can use it,
    for example, to rotate an component. Binding a root item property of speed
    to a component property of rotation would result in the item rotating in the
    screen when the simulation is run.

    To bind the root item property to a component property, select the component
    either by clicking on it on the canvas or in \uicontrol Navigator. In the
    \uicontrol Properties view, find the component property to which you want to
    bind the root item property. Select the \imageactionicon
    (\uicontrol Actions) menu next to a property, and then select
    \uicontrol {Set Binding}. In the \uicontrol {Binding Editor}, select the
    text field and enter \c {<id>.<property name>}, for example
    \c rectangle.speedProp. For more information, see \l {Setting bindings}.

    \image studio-binding-editor.png "The Binding Editor window"

    To run the simulation:
    \list 1
        \li Select the run dropdown in the \QDS top toolbar,
            and then select \uicontrol {Run App}.
        \li Select the \uicontrol Run icon in Simulink.
    \endlist
*/
